# Digital Trigger, L2-Crate power Connectors

|  |  |  |  |
| --- | --- | --- | --- |
| **usage** | **manufacturer / type** | **view** | **remark** |
| auxiliary power supply, 230VAC input at the back side of the crate | Hirschmann STASAP 2 B |  | pin usage  1 : L  2 : N  h : PE |
| +24V main power connection at the back side of the crate | Amphenol SLPRBTPSR |  | red, 4 x 8.0mm type, see below |
| +24V main power return connection at the back side of the crate | Amphenol SLPRBTPSB |  | black, 4 x 8.0mm type, see below |
| +24V main power, cable connection | Amphenol SLPRB50CPSR |  | red, 4 x 8.0mm type, see below |
| +24V main power return, cable connection | Amphenol SLPRB50CPSB |  | black, 4 x 8.0mm type, see below |