# IRIGB\_enc Firmware Properties

CPLD: XC2C64A-6VQG44C

|  |  |  |
| --- | --- | --- |
| **Revision** | **Name** | **Short Description** |
| 1 | IRIGB\_enc\_1.jed | Generates 10MHz from a 20MHz oscillator (ML602-020.0M).Generates a static IRIG-B string, first pulse is 9ms instead of 8ms for convenient scope-triggering. The static part: 191 days14 hours08 minutes32 secondsOnly the SBS-part (straight binary seconds of the day , last 200ms of the second) is dynamic, starting at 0 after power-on.Encoding:8ms = 0.1 second position identifier (start)9ms = start of the string (just for testing, should be 8ms)2ms = logic ‘0’5ms = logic ‘1’ |
|  |  |  |
|  |  |  |
|  |  |  |