# FSEB\_2, Frontplate – marking

nvent | Schroff 30848-431, 0.1 inch offset, scale 1:1

LED-holes (D=3,3) with chamfering at the back side

Letter size in 1/100 inch

FSEB.2

7

3

ESP\_P3V3

12V

12V\_over\_current

String-voltage\_in

String-voltage\_out

String\_over\_current

ESP\_Reset

String

OFF

ON

ESP

PoE

ESP

UART

8

15

12

8

8

9

9

12

9